$ cdrdao read-cd --device /dev/sr0 --read-raw --datafile "QUAKE - MS7001".bin -v 2 "QUAKE - MS7001".cue
Cdrdao version 1.2.3 - (C) Andreas Mueller <andreas@daneb.de>
/dev/sr0: PHILIPS SPD6001L	Rev: H5P2
Using driver: Generic SCSI-3/MMC - Version 2.0 (options 0x0000)

Reading toc and track data...

Track   Mode    Flags  Start                Length
------------------------------------------------------------
 1      DATA    4      00:00:00(     0)     04:12:18( 18918)
Leadout DATA    4      04:12:18( 18918)

PQ sub-channel reading (data track) is supported, data format is BCD.
Raw P-W sub-channel reading (data track) is supported.
Cooked R-W sub-channel reading (data track) is supported.
Copying data track 1 (MODE2_RAW): start 00:00:00, length 04:12:18 to "QUAKE - MS7001.bin"...
Found disk catalogue number.
Reading of toc and track data finished successfully.

